{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["NewTab","Index","DE231_1","DE231_2"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"NewTab","index":0,"n_rows":17,"n_cols":2,"rows_kept":17,"cut":false,"hidden":true,"merged":[]}
["TabTitle",{"$f":"C15","v":0}]
["Number of Tab Columns"]
["DE Starter Row Number"]
["TabSheet Starter Row Number"]
["TabSheet Header Row Count"]
["Top Header Cell"]
["Bottom Header Cell"]
["DESheet Row Count",0]
["Fixed Empty Rows",10]
["Usable Empty Rows",0]
["Total Rows Placed",0]
["Total Rows Needed",{"$f":"SUM(B8:B10)","v":10}]
["Last Tab DE Starter Row",0]
["Last Tab TabSheet Starter Row",0]
["Last Copy Starter Row",0]
["Tab Loop Number",0]
["Revision Date"]

{"sheet":"Index","index":1,"n_rows":123,"n_cols":2,"rows_kept":123,"cut":false,"hidden":true,"merged":[]}
["100-0A","1997-10-28"]
["100-1A","1997-07-15"]
["100-1B","2002-10-29"]
["100-1C","1997-07-15"]
["100-1D","2005-10-18"]
["100-4A","2002-10-29"]
["100-7","2010-04-20"]
["100-11","1998-10-27"]
["100-12","2001-04-03"]
["100-12A","1989-02-28"]
["100-13","2010-04-20"]
["100-14","2010-04-20"]
["100-15","2010-04-20"]
["100-16","2009-04-21"]
["100-17","2010-04-20"]
["100-18","2010-04-20"]
["102-3","2010-04-20"]
["102-4","2010-04-20"]
["102-5","2002-10-29"]
["102-5A","2004-04-20"]
["102-6C","2004-10-19"]
["102-10","1993-06-15"]
["102-11","2001-10-02"]
["102-12","2001-10-02"]
["102-13","1993-02-23"]
["102-13A","2002-10-29"]
["102-14","2002-10-29"]
["102-15","2002-10-29"]
["102-16","2000-10-03"]
["103-1","1981-05-22"]
["103-3","2002-10-29"]
["103-4","1998-10-27"]
["103-5","2006-10-17"]
["103-6","1981-05-22"]
["103-7","2008-04-15"]
["104-3  ","2009-10-20"]
["104-3A ","2005-04-19"]
["104-4","2009-10-20"]
["104-5","---"]
["104-5A","2010-04-20"]
["104-5B","2010-04-20"]
["104-5C","2004-04-20"]
["104-8","2006-10-17"]
["104-8A","2010-04-20"]
["104-9","2009-10-20"]
["104-10","2002-10-29"]
["104-11","2002-10-29"]
["104-12","2002-10-29"]
["105-1","1994-09-27"]
["105-3","2005-10-18"]
["105-4","2010-04-20"]
["106-1","2002-10-29"]
["106-2","2002-10-29"]
["106-3","2002-10-29"]
["106-4","1986-04-01"]
["106-5","1986-04-01"]
["106-7","1993-10-22"]
["106-8","1993-02-23"]
["107-5","1987-07-21"]
["107-7","1985-08-20"]
["107-20","1989-04-04"]
["107-21","1968-06-20"]
["107-22","1976-06-25"]
["107-23","2010-04-20"]
["107-24","2008-04-15"]
["107-25","1982-02-12"]
["107-26","1983-11-10"]
["107-27A","2001-04-03"]
["107-27B","2001-04-03"]
["107-28","2001-04-03"]
["107-29","2001-04-03"]
["107-30","2001-04-03"]
["108-1","2000-02-11"]
["108-2","1985-08-20"]
["108-2A","2002-10-29"]
["108-8A","2010-04-20"]
["108-8B","2010-04-20"]
["108-8D","2010-04-20"]
["108-9","---"]
["108-9A","2010-04-20"]
["108-11","1985-08-20"]
["108-11A","2002-10-29"]
["108-12","2000-02-11"]
["108-13A","1997-10-28"]
["108-15","1974-08-30"]
["108-16","2002-10-29"]
["108-17","---"]
["108-18","2010-04-20"]
["108-18B","2010-04-20"]
["108-22","2010-04-20"]
["108-23","1989-04-04"]
["108-23A","2002-10-29"]
["108-24","1997-10-28"]
["108-25","---"]
["108-26","1988-08-30"]
["108-26A","2002-10-29"]
["108-27","1996-04-30"]
["108-28","2006-04-18"]
["108-29","1998-04-28"]
["108-30","2010-04-20"]
["108-31","---"]
["108-32","---"]
["108-33","2008-04-15"]
["108-34","2009-10-20"]
["110-1","2005-04-19"]
["110-2","1972-10-13"]
["110-3","1985-08-20"]
["110-4","1995-03-28"]
["110-5","1972-10-13"]
["110-6","1984-06-22"]
["111-2","1989-02-28"]
["111-22","1989-02-28"]
["111-23","2002-10-29"]
["111-25","2009-04-21"]
["112-3","1971-03-19"]
["112-4","2010-04-20"]
["112-5","1980-04-18"]
["112-6","2008-10-21"]
["112-6A","---"]
["112-7","2005-10-18"]
["112-8 ","2010-04-20"]
["112-9 ","2009-04-21"]
["112-10","2010-04-20"]

{"sheet":"DE231_1","index":2,"n_rows":19,"n_cols":5,"rows_kept":19,"cut":false,"hidden":false,"merged":[[14,2,15,2],[16,4,17,4]]}
["TabTitle",{"$f":"C15","v":"PLANTING"}]
["Number of Tab Columns",1]
["DE Starter Row Number",18]
["TabSheet Starter Row Number",5]
["TabSheet Header Row Count",4]
["Top Header Cell","E15"]
["Bottom Header Cell","E18"]
["DESheet Row Count",2]
["Fixed Empty Rows",0]
["Usable Empty Rows",0]
["Total Rows Placed",2,"xlLeft",null,{"$f":"C11","v":"xlLeft"}]
["Total Rows Needed",{"$f":"SUM(B8:B10)","v":2},"General",null,{"$f":"C12","v":"General"}]
["Last Tab DE Starter Row",18,{"$f":"CELL(\"width\",C13)","v":78},null,{"$f":"CELL(\"width\",E13)","v":0}]
["Last Tab Tabsheet Starter Row",5,"A",null,"a"]
["Last Copy Starter Row",1,"PLANTING",null,"231-1"]
["Tab Loop Number",1,null,null,{"$f":"B17","v":"2011-10-18"}]
["Revision Date","2011-10-18",{"$f":"\"This Data Entry Sheet fills Tab \"&E15&\" effective \"&TEXT(B17,\"mm-dd-yy\")","v":"This Data Entry Sheet fills Tab 231-1 effective 10-18-11"},null,{"$f":"C15","v":"PLANTING"}]
["Tabulation Width",1,"Exercise all necessary caution in construction operations within"]
["Horizontal Grid Lines","No","the rest area to prevent injury to all plantings and landscaping."]

{"sheet":"DE231_2","index":3,"n_rows":125,"n_cols":5,"rows_kept":125,"cut":false,"hidden":false,"merged":[[14,2,15,2],[16,4,17,4]]}
["TabTitle",{"$f":"C15","v":"HERBICIDE"}]
["Number of Tab Columns",1]
["DE Starter Row Number",18]
["TabSheet Starter Row Number",5]
["TabSheet Header Row Count",4]
["Top Header Cell","E15"]
["Bottom Header Cell","E18"]
["DESheet Row Count",107]
["Fixed Empty Rows",0]
["Usable Empty Rows",0]
["Total Rows Placed",107,"xlLeft",null,{"$f":"C11","v":"xlLeft"}]
["Total Rows Needed",{"$f":"SUM(B8:B10)","v":107},"General",null,{"$f":"C12","v":"General"}]
["Last Tab DE Starter Row",104,{"$f":"CELL(\"width\",C13)","v":78},null,{"$f":"CELL(\"width\",E13)","v":0}]
["Last Tab Tabsheet Starter Row",95,"A",null,"a"]
["Last Copy Starter Row",91,"HERBICIDE",null,"231-2"]
["Tab Loop Number",3,null,null,{"$f":"B17","v":"2020-04-21"}]
["Revision Date","2020-04-21",{"$f":"\"This Data Entry Sheet fills Tab \"&E15&\" effective \"&TEXT(B17,\"mm-dd-yy\")","v":"This Data Entry Sheet fills Tab 231-2 effective 04-21-20"},null,{"$f":"C15","v":"HERBICIDE"}]
["Tabulation Width",1,"For all herbicide applications, the following provisions shall"]
["Horizontal Grid Lines","No","apply."]
[]
[null,null,"1. Follow all laws, rules and regulations related to the handling"]
[null,null,"of pesticides, including but not limited to: "]
[null,null,"   a. Follow all herbicide label directions, restrictions, and"]
[null,null,"precautions. "]
[null,null,"   b. The company responsible for the herbicide applicator must be"]
[null,null,"licensed with Iowa Department of Agriculture and Land Stewardship"]
[null,null,"(IDALS) as a commercial pesticide applicator company. "]
[null,null,"   c. The person applying the herbicide must be certified through"]
[null,null,"IDALS as a pesticide applicator in Category 6, Right-of-Way. For"]
[null,null,"herbicide applications that require an aquatic certification, the"]
[null,null,"applicator must also be certified as a pesticide applicator in"]
[null,null,"Category 5, Aquatics. "]
[null,null,"   d. Use herbicide and adjuvant products labeled for the"]
[null,null,"application site:"]
[null,null,"      i. For applications on the primary highway right-of-way, use"]
[null,null,"only products labeled for use on highway rights-of-way or"]
[null,null,"roadsides."]
[null,null,"     ii. For applications to or over water, use only products"]
[null,null,"labeled for corresponding use in aquatic sites, unless"]
[null,null,"intermittent pockets of standing water, such as tire ruts, and the"]
[null,null,"product is labeled for such use."]
[null,null,"    iii. For applications to areas in the water conveyance portion"]
[null,null,"of the ditch that do not contain water at the time of application,"]
[null,null,"use only products labeled for non-irrigation ditch banks or"]
[null,null,"aquatic sites."]
[null,null,"   e. Do not apply any herbicide to or over standing or flowing"]
[null,null,"water unless required coverage is obtained under a National"]
[null,null,"Pollutant Discharge and Elimination System (NPDES) Pesticide"]
[null,null,"Discharge Permit through Iowa DNR. If standing or flowing water is"]
[null,null,"encountered in areas when they need to be sprayed, notify Iowa DOT"]
[null,null,"(Roadside Development) to determine required coverage."]
[]
[null,null,"2. Schedule work according to weather conditions and take measures"]
[null,null,"to avoid off-target damage, such as runoff, leaching, drift and"]
[null,null,"volatilization."]
[null,null,"   a. Do not spray herbicide 24 hours prior to forecast"]
[null,null,"precipitation that is expected to cause significant runoff"]
[null,null,"conditions."]
[null,null,"   b. For areas with saturated soil, such as ditch bottoms, do not"]
[null,null,"spray herbicide 24 hours prior to forecast precipitation, unless"]
[null,null,"using products labeled for aquatic sites. "]
[null,null,"   c. For conventional applications, avoid applications when wind"]
[null,null,"speed exceeds 10 mph. For invert applications, avoid applications"]
[null,null,"when wind speed exceeds 15 mph. "]
[null,null,"   d. For conventional foliar applications, use a drift retardant"]
[null,null,"and maintain drift control throughout the application period by"]
[null,null,"adding more to the tank as it breaks down from agitation. "]
[null,null,"   e. Avoid spraying volatile products when temperatures are"]
[null,null,"forecast to exceed 85° F within 3 days."]
[null,null,"   f. Check the IDALS Sensitive Crops Directory and do not spray"]
[null,null,"adjacent to a listed operation when wind is blowing towards it. "]
[]
[null,null,"3. Respond to allegations of any off-target damage attributed to"]
[null,null,"handling and spraying of herbicide."]
[]
[null,null,"4. Provide the following documents to the Engineer for approval"]
[null,null,"not less than 2 weeks prior to the application. "]
[null,null,"   a. A copy of the herbicide and adjuvant labels, including any"]
[null,null,"applicable supplemental labels. "]
[null,null,"   b. A copy of the herbicide and adjuvant Material Safety Data"]
[null,null,"Sheets (MSDS.)"]
[]
[null,null,"5. Have copies of the herbicide and adjuvant labels and MSDSs"]
[null,null,"on-hand and at locations of storage, transport, and application."]
[]
[null,null,"6. Schedule work to maximize efficiency of the herbicide"]
[null,null,"application in relation to weather conditions and plant growth"]
[null,null,"stage. Follow any label recommendations given as “for best"]
[null,null,"results.” "]
[null,null,"   a. For weed applications:"]
[null,null,"      i. To determine if weeds are “actively growing,” use as a"]
[null,null,"guideline that there needs to have been at least 1 hour of"]
[null,null,"temperature above 65° F and 1 hour of sun in the day prior to, of,"]
[null,null,"or forecast before a rain the day after the application. "]
[null,null,"     ii. For spring applications to thistles, apply after basal"]
[null,null,"leaves of Canada thistles are fully extended, and after rosettes"]
[null,null,"of musk thistle are at least 8 inches diameter, but before flower"]
[null,null,"stage."]
[null,null,"    iii. For fall applications to thistles, apply prior to the"]
[null,null,"second hard freeze of 28° F, unless otherwise listed in the label"]
[null,null,"directions."]
[]
[]
[null,null,"   b. For tree and brush applications:"]
[null,null,"      i. For foliar applications and cut stump/surface"]
[null,null,"applications with water-soluble products, apply after leaves are"]
[null,null,"fully opened in the spring and prior to leaf discoloration in the"]
[null,null,"fall. "]
[null,null,"     ii. For cut stump applications with oil soluble products, do"]
[null,null,"not apply during periods of heavy sap flow. Use as a guideline"]
[null,null,"that heavy sap flow occurs in late winter to early spring when"]
[null,null,"nighttime temperatures below 32° F are followed by daytime"]
[null,null,"temperatures above 32° F with sunny conditions."]
[null,null,"    iii. For cut stump and basal bark applications, add sufficient"]
[null,null,"dye so that treated areas are visible to inspection 7 days after"]
[null,null,"application."]
[]
[null,null,"7. Notify the Engineer prior to calibrating, mixing and applying"]
[null,null,"herbicides, including incidental items."]
[null,null," "]
[null,null,"8. Provide copies of daily spray logs to the RCE at the end of"]
[null,null,"each week of spraying (form provided by Iowa DOT)."]
[]
[null,null,"9. If Contractor does not complete spray item on schedule, the"]
[null,null,"Engineer may adjust the schedule."]